**Center of Innovative and Applied Bioprocessing (CIAB)**


## Knowledge City, Sector-81 Village Molly

S.A.S Nagar, Mohali 160 306, Punjab, India

**A National Institute under the Department of Biotechnology (Govt. of India)**

**CIAB/1(61)GAP\_12/17-18/ Pur 20.02.2018**

**CORRIGENDUM**

**SUPPLY AND INSTALLATION**

**OrbitalIncubatorShaker**

### Attention is invited to the limited Tender ref no. **CIAB/1(61)GAP\_12/17-18/ Pur** for the supply and Installation Orbital Incubator Shaker. The tender opening date has been extended as:

|  |  |  |
| --- | --- | --- |
| **Tender Reference** | **As per Tender** | **Extended as** |
| **CIAB/1(61)GAP\_12/****17-18/ Pur** | Tender Opening Dated: **15.02.2018** | Extended Tender Opening Dated: **08.03.2018** |

2. The remaining specifications and term & conditions of the tender are remains same. The Chief Executive Officer, CIAB reserves the right to accept or reject any offer without assigning any reason.

S/d (Hardip Singh)

Store and Purchase Officer

बसाइट/Website : [www.ciab.res.in](http://www.ciab.res.in/) दू रभाष/Tel : 0172-5221511 फै <Rf/Fax : 0172-4990204

CIAB/1(61)-GAP-12/17-18/ N-Pur 22.01.2018

To,

NOTICE INVITING QUOTATION

Sealed Quotations are invited on behalf of Chief Executive Officer, CIAB, Mohali from reputed manufacturers/authorised distributors for the purchase of following items so as to reach latest by 14th February 2018 on or before 2.30 pm. The Quotations will be opened on the 14th February 2018 at 3.00 pm in the presence of tenderers, if any:

|  |  |  |
| --- | --- | --- |
| Sno | Description | Qty (No.) |
| 1. | Orbital Incubator Shaker**Specifications for Orbital Incubator Shaker**1. Speed: 25‐400 rpm or better
2. Scratch‐resistant transparent lid for sample viewing
3. Chamber should hold at least four or more 1L flasks
4. Temperature range of incubation from RT + 5°C to 60°C or better
5. Monitor and control chamber temperature range with ±0.1°C accuracy at 37°C
6. Should have over temperature safety feature with independent thermostat
7. Automatic restart if power is interrupted
8. Interlock stops platform when door is opened
9. Safety: audible and visible alarm in case of over/under temperature and speed
10. LED digital temperature display
11. If there is no built‐in cooling unit, an external cooling unit (i. e. a chiller) should be provided with bath volume 5 L or better and with temperature control capacity ‐20 C or better
 | 01 |

|  |  |  |
| --- | --- | --- |
|  | 12. Accessories: One universal platform; one adhesive flask mat to exactly fit the platform; clamps to hold six 125 ml, four 250 ml, four 500 ml and four 1L Erlenmeyer flasks13. European CE certified. |  |

General Conditions:

1. Copies of three PO of similar model.
2. We request you to mention the Make & Warranty period clearly in the quotation.
3. Please attach the technical literature/ leaflets/Catalogue of the quoted model/item in the bid.
4. Before quoting, please refer the instructions as per Annexure-‘1’carefully.
5. Technical compliance Sheet as per Annexure‘2’duly filled to be submitted.
6. We request you to fill the price bid format in Annexure‘3’and send the same to CIAB, Mohali

in a sealed envelope superscribing the tender ref No: by 14th February 2018 on or before 2.30

PM.

1. Offers received by E-mail/FAX will be summarily rejected.
2. Price reasonability certificate as per Annexure-4 duly filled should be submitted alongwith bid.
3. The bidders who meets the technical specification, will be considered for price comparison.
4. The tenderer should submit EMD of Rs. 8000/- in form of Bank Demand Draft favouring, Chief Executive Officer, CIAB payable at Chandigarh/Mohali. The tender without EMD will be summarily rejected.

#### Stores and Purchase Officer

**Tel: 0172-5221522**

**E-mail:** **spo@ciab.res.in**

INSTRUCTIONS

#### Annexure “1”

* Inquiry will be sent by UPC/Courier/Speed Post and CIAB will not be liable for any kind of Postal delay.
* The Quotation Should be addressed to the Executive Director CIAB, Mohali invariably giving on the envelop Reference No. With date and Due date with time.
* You should also submit the catalogue of product alongwith quotation.
* The Quantity mentioned in this inquiry and shall be deemed to be only approximate and will not in any manner be binding on the Institute.
* The quotation should be enclosed in a sealed envelope. Firms will quote separately for each article.
* The rates offered should be F.O.R Mohali.
* GST: To be quoted extra.
* In case of Ex‐godown terms the amount of packaging forwarding freight etc. should clearly be indicated by percentage or lump sum amount. Current rate of GST must be mentioned.
* The Institute is **having exemption for the payment of Excise Duty** under notification number 10/97 dated 01.03.1997 and Customs Duty under notification No.51/96 dated 23.07.1996. **Hence Excise Duty and Customs Duty, if any, should be shown separately. No other charges than those mentioned clearly in the quotation will be paid.**
* The delivery period should be specifically stated. EX‐Stock and earlier delivery may be preferred.
* The firms are requested to give detailed description and specifications together with the detailed drawings, printed leaflets and literature of the Article quoted. The name of the manufacturers and country of manufacture should also invariably be stated in the absence of these particulars the quotation is liable for rejection.
* Quotation should have minimum validity of 60 days from the date of opening.
* Late or delayed quotation will not be accepted.
* Executive Director has the right to reject to your quotations and to split up the requirements or relay any or all the above conditions without assigning any reason is reserved.
* The rates should be inclusive of installation. The payment will released after complete supply and successful installation.

**ANNEXURE ‘2’**

**FORMAT OF COMPLIANCE STATEMENT OF SPECIFICATIONS**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name of specifications/part / Accessories/Terms & Conditions of tender enquiry | Specifications of quoted Model/ Item | ComplianceWhether “YES” Or “NO” | Deviation, if any, to be indicated in unambiguous terms | Whether the compliance / deviation is clearly mentioned in technical leaflet/ literature |
| 1. Speed: 25‐400 rpm or better |  |  |  |  |
| 2. Scratch‐resistant transparent lid for sample viewing |  |  |  |  |
| 3. Chamber should hold at least four or more 1L flasks |  |  |  |  |
| 4. Temperature range of incubation from RT + 5°C to 60°C or better |  |  |  |  |
| 5. Monitor and control chamber temperature range with ±0.1°C accuracy at 37°C |  |  |  |  |
| 6. Should have over temperature safety feature with independent thermostat |  |  |  |  |
| 7. Automatic restart if power is interrupted |  |  |  |  |
| 8. Interlock stops platform when door is opened |  |  |  |  |
| 9. Safety: audible and visible alarm in case of over/under temperature and speed |  |  |  |  |
| 10.LED digital temperature display |  |  |  |  |
| 11.If there is no built‐in cooling unit, an external cooling unit (i. e. a chiller) should be provided with bath volume 5 L or better and with temperature controlcapacity ‐20 C or better |  |  |  |  |
| 12.Accessories: One universalplatform; one adhesive flask |  |  |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | mat to exactly fit the platform; clamps to hold six 125 ml, four 250 ml, four 500 ml and four 1L Erlenmeyer flasks |  |  |  |  |  |
| 13.European CE certified |  |  |  |  |

#### Annexure “3”

**PRICE BID**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| S.No. | Description | UoM | Qty | Rate | GST | Total Value |
| 1 | **Orbital Incubator Shaker**1. Speed: 25‐400 rpm or better
2. Scratch‐resistant transparent lid for sample viewing
3. Chamber should hold at least four or more 1L flasks
4. Temperature range of incubation from RT

+ 5°C to 60°C or better1. Monitor and control chamber temperature range with ±0.1°C accuracy at 37°C
2. Should have over temperature safety feature with independent thermostat
3. Automatic restart if power is interrupted
4. Interlock stops platform when door is opened
5. Safety: audible and visible alarm in case of over/under temperature and speed
6. LED digital temperature display
7. If there is no built‐in cooling unit, an external cooling unit (i. e. a chiller) should be provided with bath volume 5 L or better and with temperature control capacity ‐20

C or better1. Accessories: One universal platform; one adhesive flask mat to exactly fit the platform; clamps to hold six 125 ml, four 250 ml, four 500 ml and four 1L Erlenmeyer flasks
2. European CE certified
 | Nos. | 01 |  |  |  |

Warranty Period: -

Total bid price in Rupees

AMC Charges (in figures and words):

(after the expiry of Warranty Period)

Seal and Signature of the Bidder:

Name:

Address:

PRICE REASONABILITY CERTIFICATE

#### ANNEXURE “4”

This is to certify that we have offered the maximum possible discount to you in our Quotation No.

 dated for (Currency) .

We would like to certify that the quoted price are the minimum and we have not quoted the same item on lesser rates than those being offered to CIAB to any other customer nor they will do so till the validity of offer or execution of purchase order, whichever is later.

Seal and Signature of the tenderer